|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **conditioning tests / scope** | | | | | |
|  |  |  |  |  |  |
| **Testing in accordance with DIN EN 60115-1: 2016-03** | | | | | |
|  |  |  |  |  | clause |
| **enviromental** | |  |  |  |  |
| rapid change of temperature | | |  |  | 4.19 |
| climatic sequence | |  |  |  | 4.23 |
| damp heat steady state | |  |  |  | 4.24 |
| endurance at rated temperature (P70) | | |  |  | 4.25.1, 4.25.3 |
| operation at lower temperature | | |  |  | 4.36 |
| damp heat steady state accelerated | | |  |  | 4.37 |
|  |  |  |  |  |  |
| **mechanical** |  |  |  |  |  |
| Visual examination and checking of dimensions | | | |  | 4.4.1, 4.4.2, 4.4.3 |
| Robustness of terminations | | |  |  | 4.16 |
| Mounting |  |  |  |  | 4.31 |
| Shear (adhesion) test | |  |  |  | 4.32 |
| substrate bending test | |  |  |  | 4.33 |
|  |  |  |  |  |  |
| **eletrical** |  |  |  |  |  |
| lnsulation resistance (insulated styles only) | | | |  | 4.6 |
| Voltage proof | |  |  |  | 4.7 |
| Overload |  |  |  |  | 4.13 |
| Dangerous overload test | |  |  |  | 4.26 |
| Single-pulse high-voltage overload test | | | |  | 4.27 |
| Periodic-pulse high-voltage overload test | | | |  | 4.28 |
| Electrostatic discharge | |  |  |  | 4.38 |
| Periodic electric overload | | |  |  | 4.39 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| **additional facitilties/capabilities** | | |  |  |  |
| Drying |  |  |  |  | 4.3 |
| Temperature rise | |  |  |  | 4.14 |
| Solderability | |  |  |  | 4.17 |
| Resistance to soldering heat | | |  |  | 4.18 |
| Component solvent resistance | | |  |  | 4.29 |
| Solvent resistance of marking | | |  |  | 4.30 |
| Flammability | |  |  |  | 4.35 |
|  |  |  |  |  |  |
| **measurement capabilities** | | |  |  |  |
| Resistance |  |  |  |  | 4.5 |
| Non-linear properties | |  |  |  | 4.10 |
| Noise |  |  |  |  | 4.12 |