|  |
| --- |
| **conditioning tests / scope** |
|  |  |  |  |  |  |
| **Testing in accordance with DIN EN 60115-1: 2016-03** |
|  |  |  |  |  | clause |
| **enviromental** |  |  |  |  |
| rapid change of temperature |  |  | 4.19 |
| climatic sequence |  |  |  | 4.23 |
| damp heat steady state |  |  |  | 4.24 |
| endurance at rated temperature (P70) |  |  | 4.25.1, 4.25.3 |
| operation at lower temperature |  |  | 4.36 |
| damp heat steady state accelerated |  |  | 4.37 |
|  |  |  |  |  |  |
| **mechanical** |  |  |  |  |  |
| Visual examination and checking of dimensions |  | 4.4.1, 4.4.2, 4.4.3 |
| Robustness of terminations |  |  | 4.16 |
| Mounting |  |  |  |  | 4.31 |
| Shear (adhesion) test |  |  |  | 4.32 |
| substrate bending test |  |  |  | 4.33 |
|  |  |  |  |  |  |
| **eletrical** |  |  |  |  |  |
| lnsulation resistance (insulated styles only) |  | 4.6 |
| Voltage proof |  |  |  | 4.7 |
| Overload |  |  |  |  | 4.13 |
| Dangerous overload test |  |  |  | 4.26 |
| Single-pulse high-voltage overload test |  | 4.27 |
| Periodic-pulse high-voltage overload test |  | 4.28 |
| Electrostatic discharge |  |  |  | 4.38 |
| Periodic electric overload |  |  | 4.39 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| **additional facitilties/capabilities** |  |  |  |
| Drying |  |  |  |  | 4.3 |
| Temperature rise |  |  |  | 4.14 |
| Solderability |  |  |  | 4.17 |
| Resistance to soldering heat |  |  | 4.18 |
| Component solvent resistance |  |  | 4.29 |
| Solvent resistance of marking |  |  | 4.30 |
| Flammability |  |  |  | 4.35 |
|  |  |  |  |  |  |
| **measurement capabilities** |  |  |  |
| Resistance |  |  |  |  | 4.5 |
| Non-linear properties |  |  |  | 4.10 |
| Noise |  |  |  |  | 4.12 |